1.02.00 EULA reset, factory defaults on reset pin, serial number format, icons
1.03.00 Default site setup uses Q-Sys web file, new emsetup defaults
1.05.00 Anti echo work, work on rate limiting on faders
1.07.00 Added duplicate detection on Symetrix, Q-Sys site setup items
1.09.00 Up device serial length to 13, LED test
1.13.00 Fixed date month, add sleep timeout option, up TCP MSS and Win size
1.13.05 Added speed test, fixed Wireshark corruption, Win size fiddling, CLI CPU work, Syslog PHY
1.13.08 Updated FreeRTOS+TCP to 2.3.3
1.14.01 Startup with dark screen, internal task optimization to fix task starving, FC4X top row buttons
        Web defaults limits on Q-Sys, CLI updates, reboot repair
1.14.02 Russian titles, UTF-8 safe copy
1.14.04 Daughterboard debugging on console, update firmware fix
1.14.10 Fixed leaking network buffers, netstat, logging, improved Symetrix aspects
1.14.12 Fixed default static IP address
1.15.03 Added support for Rev2 daughterboard
1.15.04 Added custom fader scaling for Q-Sys
1.15.05 Increases Biamp instance ID maximum length to 12 characters
1.16.01 Added dark mode, Tesira link troublshooting helpers, increases Biamp instance ID maximum length to 16 characters, support for Q-Sys plugin (v1.5) channel and Control labels, crash logging, rename DSP communication error. Bug fixes: Hide unsupported DSP type, fix LED test causing displays to flash.
1.16.10 Added level option to Tesira alt faders
1.17.00	Add SSH communication
1.17.10 WolfSSH patched, malloc fail reporting
1.17.20 Added to slow heap, changed HTTP buffer sizes
1.17.25 Added detailed logging to buffer fail, HTTP timeout at 2 minutes, multicast filter at MAC
1.17.30	Fix issue with channel naming on bank 2